------------------------------------------------------------------------------------------
+			        BIOS History for MS-B907                                    +                  
------------------------------------------------------------------------------------------
8XX For Intel Kabylake B250 + NCT6685 + DDR4 SO-DIMM*2  PCB 1.0  ERP: 606-B9071
------------------------------------------------------------------------------------------
BOM SIO(SB) GPIO:           
   GPIOXX      GPIOXX       GPIOXX                 market name                     ERP                     PCB
    XX           XX            XX                      XX                          XX                      XX
    XX           XX            XX                      XX                          XX                      XX
=========================================================================================
Flash Tool:
!!!The first time flashing BIOS at manufactory, 
   You can use flash tool FPT.EXE;
EX: C:\FPT /F EAC17IMS.YYY
!!!The end user want to update system BIOS to fix some bugs,  
   You can use flash tool .
EX: 
================= System Information =====================================================
Product Model   : MS-B907
System Platform : Intel Kabylake
Processor       : Kabylake
SouthBridge     : Kabylake B250
SuperI/O Chip   : NCT6685
SSID		: 0x1462B907 
Audio SSID (opt): 0x1462B907
Setup Engine    : GSE Setup

================ OptionRom/Firmware Information ==========================================
GOP             : 1054 
VBIOS           : 1046 
ME Version      : 11.6.26.1246 
RAID ROM        :  
LAN OptionRom   :  
Device OptionRom:

================ Reference Code Information ==============================================
MRC version     : 170_029 
AMI BaseCode    : 5.12_VEB_1ATQP029 

================ Flash Tool Information ==================================================
FPT Version     :  
AFUDOS Version	: 

================ MicroCode Information ==========================================
CPUID 	uCode PlatformID
----- 	----- ----------

M36506E3_000000BA      Intel(R) Skylake Processor N-0 (Skylake-H) 
M2A906E9_0000005E      Intel(R) KabyLake Processor B-0 (Kaby Lake-H)
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.920 					                                   Build Date: 2017/08/28
Old Version: EB907IMS.921
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: 9FC4h        

Description for FAE:
01. Release MP BIOS
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.921 					                                   Build Date: 2017/08/17
Old Version: EB907IMS.910
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: 0FDAh       

Description for FAE:
01. Fix auto lan boot (IPV4/6) fail without any device can be boot up.
02. Update Intel MicroCode M36506E3 BA for SKL-H cpu & M2A906E9 5E for KBL-H cpu.
03. Modify issue about auto enter bios setup when legacy network boot priority earily than Hard disk in dual mode.  
04. According new SPB spec ,project not support SMART HDD function
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.910 					                                   Build Date: 2017/07/10
Old Version: EB907IMS.912
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: C08Ah     

Description for FAE:
01. Release MP BIOS
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.912 					                                   Build Date: 2017/06/26
Old Version: EB907IMS.911
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: 49DAh   

Description for FAE:
01. Update RST pre OS 15.7.0.3054.
02. Modify Remove Optane Device cause BIOS Boot Mode change to ¡§Legacy+UEFI¡¨ from ¡§UEFI¡¨.
03. Modify HARDWARE MONITOR temperature unit.
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: JinmeKuo
New Version: EB907IMS.911 					                                   Build Date: 2017/06/12
Old Version: EB907IMS.900
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: A595h  

Description for FAE:
01. Modify DRAM which installed DIMM2 slot will show Unknown string after clear cmos.
02. Modify Optane Genie item default value to Disabled.
03. Modify Optane function.
04. Patch S3 fail issue.

*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.900 					                                   Build Date: 2017/05/15
Old Version: EB907IMS.903
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: DA77h            
      
Description for FAE:
01. Release MP BIOS
02. Take old way (set SSC to 0) to patch issue - [B907_w10]Sometimes ODD device lost¡Aafter reboot will be ok   
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.903 					                                   Build Date: 2017/05/05
Old Version: EB907IMS.902
Codebase: AioSpec_Obm050_035 / CRB029 
RC Code: 1.7.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.26.1246
CheckSum: EB33h            
      
Description for FAE:
01. Hidden Optane mode for version 8xx BIOS
02. Modify display not correct when F11 boot to ODD ,but not press any key.
03. Update codebase to AioSpec_Obm050_035 (CRB029 / RC 1.7.0)
04. Update ME to version 11.6.26.1246 from 11.6.0.1126
05. patch cannot display Plextor SSD information in setup.
06. Fix Sometimes the BIOS display not correct.
07. Add new solution for issue as below
    495932 - [B907_w10]Sometimes UUT show blackscren when press ¡§del ¡¨ key¡Adebug code¡GA1
    491401 - [B908_w10]Sometimes UUT show blackscren when press ¡§del ¡¨ key¡Adebug code¡GA1
    493249 - [B090_w10]Sometimes UUT show blackscren when press ¡§del ¡¨ key¡Adebug code¡GA1
    493248 - [B090_w10]Sometimes UUT show blackscren when press ¡§del ¡¨ key¡Adebug code¡GAb
    490446 - [B908_W10]UUT will show blackscreen about 4s after enter the BIOS password    
08. Modify DMI_RECOVERY_BLOCK_ADDRESS for GSE and Lite model platform.
09. Modify BIOS execute disable bit show N/A
10. Modify Help page should modify in Hardware Monitor.
11. Modify Both of "Full Screen Logo Display" and "Bootup NumLock State" all should be hidden.
12. Show Optane mode for version 9xx BIOS & set M2Genie_SUPPORT Enabled
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.902 					                                   Build Date: 2017/04/17
Old Version: EB907IMS.901
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.0.1126
CheckSum: DF86h            
      
Description for FAE:
01. Modify firmware update support
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.901 					                                   Build Date: 2017/04/12
Old Version: EB907IMS.820
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.0.1126
CheckSum: F9D2h           
      
Description for FAE:
01. Set SATA Mode default to Intel RST With Intel Optane System Acceleration and update RST RAID driver to 15.5.0.1051
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.820 					                                   Build Date: 2017/02/15
Old Version: EB907IMS.825
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.0.1126
CheckSum: AE94h          
      
Description for FAE:
01. Release MP BIOS
02. Modify SMBIOS Type01 "System Family" & "SKU Number" to follow new spec. with MSFT MDA3 tool test. 
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.825 					                                   Build Date: 2017/02/09
Old Version: EB907IMS.824
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.0.1126
CheckSum: AA5Dh      
      
Description for FAE:
01. Modify issue - 495932 - [B907_w10]Secure boot Support&Network stack default value is disabled after Clear CMOS.	
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.824 					                                   Build Date: 2017/01/05 
Old Version: EB907IMS.823
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS: 1046                         GOP: 1054                          ME: 11.6.0.1126
CheckSum: 97D1h     
      
Description for FAE:
01. Modify System Explorer by each project
02. Add Language button to support multi language
03. Downgrade ME to version 11.6.0.1126 from 11.6.1.1142
04. Modify issue - 490179 - [B907_w10]UUT show blackscreen when run S4 , debug code:04,4s shutdown
05. Modify issue - 493488 - [B907_w10]U4 do reboot when run S4 31counts¡]after run S3 30counts¡^ 
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.823 					                                   Build Date: 2016/12/20 
Old Version: EB907IMS.822
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS  : 1046                       GOP    : 1054
CheckSum: 04AEh    
      
Description for FAE:
01. Modify issue - 494584 - [B907_w10]Type C port show USB3.1 Gen 2 in System Explorer
02. Modify DMI data and password (Password Clear Disabled) should be keep value after clear cmos
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.822 					                                   Build Date: 2016/12/14 
Old Version: EB907IMS.821
Codebase: AioSpec_Obm035_026 / CRB022 
RC Code: 1.3.0
VBIOS  : 1046                       GOP    : 1054
CheckSum: 46F6h   
      
Description for FAE:
01. Take new way (set ZPODD ASL code implement) to patch issue - [B907_w10]Sometimes ODD device lost¡Aafter reboot will be ok   
02. Update codebase to AioSpec_Obm035_026 and remove unnecessary function
03. Update Intel Microcode M22906E9_00000048
04. Fix can't boot AHCI legacy os or pendrive
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.821 					                                   Build Date: 2016/12/09 
Old Version: EB907IMS.810
Codebase: AioSpec_Obm032_023 / CRB022 
RC Code: 1.3.0
VBIOS  : 1046                       GOP    : 1054
CheckSum: B231h  
      
Description for FAE:
01. Update codebase to AioSpec_Obm032_023
02. Support F3 recovery key for Win10
03. Cancel Update VBIOS 1047 & GOP 1056
04. Cancel Modify issue - 491412 - [B907_w10]Press ¡§del¡¨ key can boot to BIOS after resuming from S4
05. Modify issue - 492439 - [B907_w10]Temperature unit display is not correct in BIOS hardware monitor page	
06. Modify SYS Fan depend on Temperature Src0 with "Nuvoton PC Health Manager Pro" HWM tool
07. Update ME to version 11.6.1.1142 from 11.6.0.1126
08. Fix intel 600P PCIe SSD will lose boot device after run burn in test.
09. Patch - Boot priority sometimes change the order automatically
10. Take new way to modify PCIE SSD information
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.810 					                                   Build Date: 2016/12/07
Old Version: EB907IMS.811
Codebase: AioSpec_Obm024_015 / CRB017 
RC Code: 1.0.4
VBIOS  : 1046                       GOP    : 1054
CheckSum: 0812h   
      
Description for FAE:
01. Release MP BIOS

*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.811 					                                   Build Date: 2016/12/06
Old Version: EB907IMS.800 
Codebase: AioSpec_Obm024_015 / CRB017 
RC Code: 1.0.4
VBIOS  : 1046                       GOP    : 1054
CheckSum: A2E0h 
      
Description for FAE:
01. Patch - Boot priority sometimes change the order automatically
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.800 					                                   Build Date: 2016/11/30 
Old Version: EB907T01.80D (TEST BIOS)
Codebase: AioSpec_Obm024_015 / CRB017 
RC Code: 1.0.4
VBIOS  : 1046                       GOP    : 1054
CheckSum: C55Bh 
      
Description for FAE:
01. Release MP BIOS
02. Modify SYS Fan depend on Temperature Src0 with "Nuvoton PC Health Manager Pro" HWM tool
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907T01.80D (TEST BIOS)                                  Build Date: 2016/11/29
Old Version: EB907IMS.80D
Codebase: AioSpec_Obm024_015 / CRB017 
RC Code: 1.0.4
VBIOS  : 1046                       GOP    : 1054
CheckSum:  

Description for FAE:
== EB907IMS.80E ==
01. Add Board Explorer function
02. Modify SB GPIO table
03. Update Intel Microcode M22906E9_00000042 for B-0 stepping processor
== EB907IMS.80F ==
01. Modify issue - 492759 - [B907_w10]WHQL test fail (usb exposed system test fail)	
02. Modify issue - 491154 - [B907_w10]Sometimes UUT show blackscren when press ¡§del ¡¨ key¡Adebug code¡GA1

03. According MB DIMM information ,bios DIMM information need to be modify DIMM1/DIMM2.
04. Modify issue - 493175 - [B907_w10]Please add system fan curve in BIOS
05. Modify ME setting
== EB907IMS.80G ==
01. Modify issue - 493127 - [B907_w10]UUT hang debug code¡G62 after press power button 10s clear CMOS
02. Modify RTC can't wake when press power button to shutdown
03. Disable PS/2 wake function by HW request
04. Patch issue - 490974 - [B907_w10]Sometimes uut auto wake up from S3 and PS/2 mouse has no function	
05. Modify Board Explorer function
06. Patch issue - [B907_w10]Sometimes ODD device lost¡Aafter reboot will be ok   
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.80G 					                                   Build Date: 2016/11/25
Old Version: EB907IMS.80F
Codebase: AioSpec_Obm030_021 / CRB022 
RC Code: 1.3.0
VBIOS  : 1047                       GOP    : 1056
CheckSum: 7C48h 
        
Description for FAE:
01. Modify issue - 493127 - [B907_w10]UUT hang debug code¡G62 after press power button 10s clear CMOS
02. Modify RTC can't wake when press power button to shutdown
03. Disable PS/2 wake function by HW request
04. Patch issue - 490974 - [B907_w10]Sometimes uut auto wake up from S3 and PS/2 mouse has no function	
05. Modify Board Explorer function
06. Patch issue - [B907_w10]Sometimes ODD device lost¡Aafter reboot will be ok   
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.80F 					                                   Build Date: 2016/11/21
Old Version: EB907IMS.80E
Codebase: AioSpec_Obm030_021 / CRB022 
RC Code: 1.3.0
CheckSum: 0BDAh        
Description for FAE:
01. Modify issue - 492759 - [B907_w10]WHQL test fail (usb exposed system test fail)	
02. Modify issue - 491154 - [B907_w10]Sometimes UUT show blackscren when press ¡§del ¡¨ key¡Adebug code¡GA1
03. According MB DIMM information ,bios DIMM information need to be modify DIMM1/DIMM2.
04. Modify issue - 493175 - [B907_w10]Please add system fan curve in BIOS
05. Modify ME setting
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.80E 					                                   Build Date: 2016/11/16
Old Version: EB907IMS.80D
Codebase: AioSpec_Obm030_021 / CRB022 
RC Code: 1.3.0
CheckSum: FD03h      
Description for FAE:
01. Add Board Explorer function
02. Update codebase to AioSpec_Obm030_021 
03. Update Intel Microcode M22906E9_00000042 for B-0 stepping processor
04. Update VBIOS 1047 & GOP 1056
05. Modify issue - 491412 - [B907_w10]Press ¡§del¡¨ key can boot to BIOS after resuming from S4
06. Modify issue - 492439 - [B907_w10]Temperature unit display is not correct in BIOS hardware monitor page	
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.80D 					                                   Build Date: 2016/11/08
Old Version: EB907IMS.80C
Codebase: AioSpec_Obm024_015
CheckSum: 8C62h    
Description for FAE:
01. Modify issue - 492440 - [B907_w10]The upper right corner of the BIOS screen shows a line.	
02. Modify issue - 489974 - [B907_w10]Cannot detect M.2 SATA SSD information
03. Modify B907 fan curve for thermal request
04. Remove unnecessary function and modify ME / eSIO setting
05. Does not support A-0 stepping processor         
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.80C 					                                   Build Date: 2016/11/01
Old Version: EB907IMS.80B
Codebase: AioSpec_Obm024_015
CheckSum: 145Dh   
Description for FAE:
01. Modify issue - 491829 - [B907_w10]Suggest remove"Entering Boot Menu...."on CPU and System fan error menu
02. Hidden Intel RST With Intel Optane System Acceleration until UEFI driver ready
03. Modify issue - 491910 - [B907_w10]SLP 2.0 test fail 
04. Remove unnecessary item and unnecessary private file
05. Fix S3 resume SMBUS address Incorrect
06. Support multi language
*=========================================================================================*
Model: MS-B907 	 			              PCB: 1.0         	                 Author: StanleyChung
New Version: EB907IMS.80B 					                                   Build Date: 2016/10/25 
Old Version: EB907IMS.80A
Codebase: AioSpec_Obm024_015
CheckSum: 7331h  
Description for FAE:
01. Modify issue - 489340 - [B907_w10]BIOS SW1 Function not ready
02. Modify issue - 488890 - [B907_w10]Sometimes BIOS Menu show¡§ROM Image is not loaded¡¨ and¡§ROM Image update denied¡¨             
03. Cancel "M2 RST Pcie Storage Remappin" (RAID) default is Enable.
04. Set REQ6/10 to disable for TL-673 by HW request
05. Set Charge_CB to 1 (not charge) when Sx resume by HW request
06. Add setup item "Chassis Intrusion Configuration" for JCO1 CaseOpen function
07. Modify user password to entry BIOS , the "Trusted computing" still can be modified.
08. Modify firmware update support and update module to v.07 from v.06
09. Update DMIControlDefault module to v.09 from v.07
10. Modify issue - 490974 - [B907_w10]Sometimes uut auto wake up from S3 and PS/2 mouse has no function
11. Modify issue - 491775 - [B907_w10]Seggest change Baseboard Version from "0B" to "1.0"
12. Modify issue - 491771 - [B907_w10]Suggest remove "XMP" Function in BIOS
13. Modify SB GPIO porting
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.80A 					                                   Build Date: 2016/10/18
Old Version: EB907IMS.809
Codebase: AioSpec_Obm024_015
CheckSum: 0E0Ah 
Description for FAE:
01. Update codebase to AioSpec_Obm024_015
02. Update ME to version 11.6.0.1126 from 11.6.0.1117   
03. Support Intel RST With Intel Optane System Acceleration
04. Modify firmware update support.
05. Modify issue - 490363 - [B907_w10]Set AC power loss as power on,uut cannot power on when replug power cord
06. Suggest "M2 RST Pcie Storage Remappin" (RAID) default is Enable.            
07. Modify VBIOS & GOP setting (Disable LFP EDID support)
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.809 					                                   Build Date: 2016/10/12
Old Version: EB907IMS.808
Codebase: AioSpec_Obm020_013
CheckSum: A4ECh
Description for FAE:
01. Add firmware update support.
02. Modify issue - 489475 - [B907_w10]V803 system BIOS cannot flash¡A show error info
03. Modify issue - 490099 - [B907_w10]Cannot Flash DPK,show "Inject DPK Fail"	
04. Modify SMBIOS data location in NVRAM and remove unnecessary private file
05. Modify NVME PCIE SSD information on EZ MODE
06. Modify issue - 490420 - [B907_w10]Boot Override display incomplete when select this item in BIOS
07. Update GOP to ver.1054 and Modify GOP(1054) & VBIOS(1046) setting 
08. Update Realtek ALC1150 VerbTable for B907 0B Motherboard           (HDACfg-0900-1462B907.MSB9070B.0x14Single.EAPED.GPIO0.I2S0x1B.161003.txt)
09. Modify "MB: MS-B907" change to "Product: B250 Gaming Aegis 3(MS-B907)" on BIOS Main page   
10. Modify AC Power loss for Deep S4/S5
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.808 					                                   Build Date: 2016/10/05
Old Version: EB907IMS.807
Codebase: AioSpec_Obm020_013
CheckSum: 0EFDh
Description for FAE:
01. Modify "MB: MS-B907" change to "Product: B250 Aegis 3(MS-B907)" on BIOS Main page   
02. Modify issue - 490414 - [B907_w10]Suggest change Product Name to B250 Aegis 3(MS-B907)
03. Modify EZ mode (Delete CPU GT Voltage / Memory DIMM3)
04. Modify Trusted Computing default setting. (Hidden Device Select and unnecessary item / Tune TPM Device Selection item postition)
05. Support XMP Function.
06. Modify RTC Alarm help string.
 
07. Modify issue - 490413 - [B907_w10]CPU IO/CPU SA show 0.000V in BIOS INFO menu
08. Modify issue - 489098 - [B907_W10]F1/DEL/ESC keys have no function under S.M.A.R.T prompt message interface.
09. Modify DVMT size (return default) and unnecessary microcode
10. Update codebase to AioSpec_Obm020_013 and modify SIO NCT6685D Module version to 01.
11. Modify issue - 488936 - [B907_w10]installing VGA card then power on,sometimes the system automatically shut down
12. Modify issue - 488931 - [B907_w10]sometimes system hang up in msi logo after install VGA card,debug code show A2
13. Update ME to version 11.6.0.1117 from 11.6.0.1109   
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.807 					                                   Build Date: 2016/09/29
Old Version: EB907IMS.806
CheckSum: 37C1h     
Codebase: AioSpec_Obm018_010
Description for FAE:
01. Modify issue - #489921 - [B907_w10]There is no IPV6 in the boot menu/boot priorities.	 
02. Modify issue - #489078 - [B907]ludashi(¾|¤j®v) show "MS-B907 All in One"information
03. Modify issue - #489092 - [B907_w10]Unplug CPU/system fan,UUT does not display warning message
04. Modify to Suggest hidden some items in Trusted Computing interface  
05. Modify AC loss Function work and setup Item(M.2)
06. Modify issue - 490363 - [B907_w10]Set AC power loss as power on,uut cannot power on when replug power cord
07. Modify issue - 490362 - [B907_w10]Set AC power loss as last state,uut cannot power on when replug power cord
08. Modify issue - 489103 - [B907_W10]Prompt info show garbage characters after set up Favorites in Default Homepage.
09. Modify issue - 489091 - [B907_W10]Prompt message display incomplete after enter three times wrong password.
10. Modify Default HomePage of Favorite setting behavior is incorrect. 
11. Modify issue - 489256 - [B907]The speed of PCIe SSD is only about 820MB/s,will be ok after resuming from S3/HS3
12. Modify issue - 489264 - [B907_w10]The speed of PCIe SSD will down when test two SSD together
13. Modify issue - 490416 - [B907_w10]Suggest change Type in Type 03 to Desktop
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.806 					                                   Build Date: 2016/09/21
Old Version: EB907IMS.805
CheckSum: F15Fh  
Codebase: AioSpec_Obm018_010  
Description for FAE:
01. Modify issue - #490117 - [B907_w10]charge function abnormal after resume acpi                  
02. Add a token to lock Nuvoton ESIO EC Space Page 1 to avoid other tool modify setting.
    Default = Enable (lock) 
03. Modify issue - #489678 - [B907_w10]Run Performance Assessment Toolkit, Fast Startup test fail  
04. Update Intel Microcode M22906E9 3A for B-0 stepping processor & support A-0 stepping processor
05. Modify Smart Fan Function to fix CPU Fan show 0 RPM in Hardware Monitor
06. Modify issue - #489143 - [B907_w10]Manufacturer String display not complete                    
07. Remove "Wake Up Event By" item by AIO SPEC.
08. Modify Favorites Setting and Remove DDR Voltage by AIO SPEC.  	   
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.805 					                                   Build Date: 2016/09/12
Old Version: EB907IMS.804
CheckSum: 8348h   
Codebase: AioSpec_Obm018_010
Description for FAE: 
01. Update VBIOS 1046 & GOP 1052 ,And modify Hot plug monitor behavior   
02. Modify USB KB & MS should not be wake from S4 when EUP2013 disabled (follow AIO SPEC)
03. Enable OC support.
04. Modify issue - #489083 - [B907]cpu speed show 0.00GHz in bios setup		
05. Modify issue - #489081 - [B907]Vcore show 0.272~0.288V in bios setup
06. Modify issue - #489080 - [B907]Memory size show 0MB in BIOS setup
07. Modify issue - #489079 - [B907]memory speed show "0MHz" in bios setup
08. Modify DVMT size & board setting
09. Modify issue - #489355 - [B907_w10]The label of SATA port in BIOS is difference from MB
10. Modify ME setting & fix hang 0x15 for 0B Motherboard
11. Hide Build in shell in UEFI mode
12. Disable serial com port 1 (COMA) Present by HW request
13. Modify PCB version to 0B
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0B          	                 Author: StanleyChung
New Version: EB907IMS.804 					                                   Build Date: 2016/09/07
Old Version: EB907IMS.803
CheckSum: 1449h  
Codebase: AioSpec_Obm018_010
Description for FAE:    
01. Enable onboard lan work (Killer E2500)
02. Modify issue - #489173 UUT will auto wake up when do S4
03. Modify serial com port 1 (COMA) Present by HW request               
04. Update Realtek ALC1150 VerbTable for B907 0B Motherboard (HDACfg-0900-1462B907.MSB9070B.0x14Single.EAPED.GPIO0.I2S0x1B.160902.txt)
05. Modify PS/2 Function work
06. Update codebase to AioSpec_Obm018_010
07. Update ME to version 11.6.0.1109 from 11.6.0.1102
08. Modify issue - #489084 Suggest add PCIE SSD information            	
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0A          	                 Author: StanleyChung
New Version: EB907IMS.803 					                                   Build Date: 2016/08/31
Old Version: EB907IMS.802
CheckSum: E67Ah  
Codebase: AioSpec_Obm012_005
Description for FAE:
01. Update ME to version 11.6.0.1102 from 11.6.0.1055
02. Hidden "AUTO CLR_CMOS" item in bios setup
03. Modify NCT6685D EUP Function
04. Modify issue - #489137 Suggest "EuP 2013" default set enable 
05. Modify platform setting & hidden unnecessary function
06. Modify issue - #488979 System status has no EC version in BIOS
07. Modify SB GPIO setting (GPIO/Multifunction/Unuse)
08. Modify issue - #489101 Suggest hidden some items in Trusted Computing interface
09. Initial power LED when S3 resume by HW request
10. Modify issue - #489047 suggest "security device support" default set enable
11. Disable auto fix stop bit function support by bios
12. Modify board Lan switch control
*=========================================================================================*
Model: MS-B907 	 			              PCB: 0A          	                 Author: StanleyChung
New Version: EB907IMS.802 					                                   Build Date: 2016/08/24
Old Version: EB907IMS.801
CheckSum: 7C2Ch  
Codebase: AioSpec_Obm012_005
Description for FAE:
01. Modify ME setting by HW request.
	  Platform IMON Disable set to 0x01 (It cause system hang on 0x63)
02. Disable EC Auto fix reg.   (It cause system auto shutdown)
    (Page0x07, Index 0x17 , BIT6 set to 1)
03. Update codebase to AioSpec_Obm012_005
04. Modify platform can't boot or install OS.    
05. Modify platform setting
06. Modify PS/2 Function work
07. Add Super Charger function.
08. Modify Issue #488799 - PCI memory controller show yellow mark in device manager.
09. Fix PS2 device can not wake up in S3.
10. Modify AC POWER LOSS function
11. Update Realtek ALC1150 VerbTable
12. Modify unuse SB GPIO setting 
13. Modify global register depend on eSIO F/W control.

*=========================================================================================*
Model: MS-B907 	 			              PCB: 0A          	                 Author: StanleyChung
New Version: EB907IMS.801 					                                   Build Date: 2016/08/03
Old Version: 
CheckSum: 4CE6h 
Codebase: AioSpec_Obm008_004
Description for FAE:
01. Base on KBL AioSpec_Obm008_004 Initial bring up version.
02. Fill in B907 SSID & SVID (0xB9071462)
03. Update Realtek ALC1150 VerbTable
04. Update ME 11.6.0.1055 setting
05. Modify bios version & building name
06. Switch to GSE interface.
07. Disable OC & M-Flash support
08. Modify Win10 Firmware capsule update & guid
09. Add NUVOTON NCT6685D SIO Module
10. Add a token to lock Nuvoton ESIO EC Space Page 1 to avoid other tool modify setting.
    Default = Disable (Don't lock)
11. Modify VBIOS 1040 & GOP 1046   
12. Enable PS/2 Function.
13. Modify eSIO Nuvoton NCT6685D GPIO 
14. Modify SB GPIO
15. Modify INTEL/WGI219V LAN


*=========================================================================================*





         